SEAWOLF PILOTHOUSE 36
“Full Circle” STC 36058L607

HULL SPECIFICATIONS:


Length
 

35’11”


Beam
 

11’2”


Deadrise aft
14 degrees


Deadrise fwd
35 degrees


Bottom

.250” 5086 Aluminum


Sides and bulkheads
.190” 5086 Aluminum


Side Height aft
51.5”


Decks


.190” 5052 Aluminum (Treadplate)


Cabin sides and bulkheads
            .160” 5052 Aluminum


Cabin roof

            .125” 5052 Aluminum

Weight, dry with twin D6 310            13,550 lbs


Performance, wet, loaded, top speed 39 knots


Propulsion:


2-Volvo Penta D6 310 diesel Duoprop I/O


EVC Electronic Vessel Control


Instrument panels with EVC engine and fuel data, tachometer, hourmeter, 



engine temp, oil pressure, fuel level, voltmeter, drive trim gauge 



and wiring harness



Fresh water cooling



2-Racor 500 water separating fuel filter



Volvo electronic engine controls (three station)



Teleflex hydraulic steering, with engine power assist


Engine compartment sound insulation


Bow Thruster ; Sidepower 100/185 with 3 station control
Full Circle STC 36058L607
(cont.)


Hull, general:



Cockpit deck, flush, self-draining



Bowrails and cockpit handrails 1” s-40 aliminum pipe, welded



Cabin top handrails, 1” aluminum pipe, welded



Radar arch, 1 1/2”aluminum pipe, welded, with antenna and GPS mounts



Anchor roller, ¼” plate, welded, with 3” roller 



Anchor rode locker, with drains and access hatch 



Swimstep, 28” welded, with welded transom grab handles


Cleats, seven 10” cast aluminum, welded


Fairlead chocks ,cast aluminum, welded



Engine hatches, two, with gas lifting struts



Storage holds, two, self draining, under cockpit deck 60”L x 30”W x 15” D


Fuel tank, one, 252 gallon, bolt in w/gauge sender



Fuel tank access, bolt down plate on deck to access entire fuel tank



Fuel tank quick access, Fraser 8” cast aluminum access hatch on deck



Bilge pumps, 3-Jabsco 3700 GPH w/automatic float and panel switches



Trim-tab system, Boat Leveler 12" x 18" 


Running lights, Aqua Signal series 20



Horn, AFI 10029 XLP electric dual trumpet 


Deck light, Jabsco 4"x 6" halogen mounted on mast



Windlass; Lewmar 1000H electric, with deck mount foot switches



Doors and windows, All heavy duty aluminum frame Diamond /Seaglaze 




With ¼” tempered glass



Extensive acoustic insulation throughout



1-Zinc anode on hull



Large comfortable finished forecabin



Quiet, comfortable pilothouse style main cabin



All interior stick built, with structural aluminum welded in place 
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Electrical System DC;



Batteries, house, 4- GC 145 6 Volt Deep cycle (490 amp hours)



Battery, engine, one gp 31HD 1025 CCA 



Battery switches, BEP heavy duty with emergency parellel 



Automatic charging relay, Blue Sea Systems



Main DC circuit breakers, Blue Sea Systems 185 series



Electrical panels, 2-Blue Sea Systems 8023 with 8 toggle circuit breakers each



Dash switch panel, 10 Contura rocker switch with push-to-reset circuit breakers



12V DC outlet, one at dash



Wiring, all fine stranded marine grade duplex tinned copper



Connectors and fittings, all “Ancor” marine grade 


Electrical System AC;


Shore power system, 30 Amp,



Power inlet, Marinco 303 ELB



Shore power cord, 50' Marinco



Electrical panel AC, Blue Sea 8027 with main breaker, polarity indicator 




and 5 toggle breakers for branch circuits



Electrical outlets, 4- duplex, one in forcabin, one at galley and one at dinette,



One at companion seats



Shore power Isolation transformer, Charles IXFMR 30



Genset; Northern Lights M673D 6kw with sound enclosure




Standard S-1B start/stop panel with hour meter and preheat




50A/30A ship-shore transfer switch



Inverter/Charger; Magnum Energy 28/12/100 with battery monitor panel


All fine stranded marine grade triplex tinned copper wire



All Ancor marine grade connectors and fittings


Fresh Water System;



Fresh water tank, 68 gallon,aluminum, bolt in



Fresh water pump, Jabsco Sensor Max 4.5 gpm (or similar) automatic



Galley sink, Polar stainless, single 9”deep 



Galley faucet, Skandvic 10488 single lever 



Water heater, Seaward 11 gallon heat exchanger/ 120 volt



Shower drain system, Attwood 4143-4 automatic
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Head:



Toilet, VacuFlush system


Holding tank, Sealand 28 gallon heavy duty rotomolded plastic




With vent filter system and tankwatch monitor



All fittings and penetrations on top of tank



Waste discharge pump, Sealand T-12 electric diaphragm



Deck discharge for dockside vacuum system



Sink, Polar stainless, oval with Scandvic combination faucet/shower



Shower drain system



Waterproof self retracting toilet paper holder



Storage cabinet with teak louvered door

Cabin / Interior;

Forecabin 8’4”length: 



King berth (6’4” x 6’8”) with 6” upholstered cushion



Hanging locker starboard with one drawer under




Storage shelf port, starboard and forward with carpet liner and teak trim



One storage locker each side with sliding doors, shelf, carpet liner and teak trim



Portlites, 4-Lewmar Ocean series, opening with screens



Skylight hatch, Bomar 1029-10 with screen



Panel headliner with acoustic foam insulation



Cabin lights, 2-red / white



Access to anchor locker



Heavy duty rubber flooring



Marine carpet hull liner 



Head compartment portside, painted




Teak entry door with Perko latch with lock




Storage locker with teak louver door




Toilet paper holder, waterproof, self retracting




Stainles grab bars




Light, red / white


Main cabin, pilothouse style, 10’8” length;



Helmstation starboard side with teak dash and console


Helmseat, Bentleys Rivermaster with folding armrests on Garelick slide



Storage cabinet, under helmseat with one shelf and door



Storage, open under helm floor



Storage, cabinet below galley sink with one shelf and door
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Cabin / Interior cont.



Nova-Kool 7.5 two door refrigerator/ freezer




3 storage drawers




Hanging locker




Stove, ENO 3 burner propane with propane system including




2-1.4 gallon aluminum tank



Dinette portside, includes;




Table, 30”x 46”with teak sea rail




Dinette converts to berth 46”x 73”




Bench seats, face to face with storage under with top access




Dinette cushions 4”



Companion seats forward, 2-Bentleys Rivermaster with folding armrests 




Storage, under companion seats with chart storage tubes



Storage, under companion floor with top access




Storage, 4 huge 16”x 30” x9” drawers under dinette 


Furnace, Webasto TSL17 17,000 BTU Hydronic


Air conditioning; Carrier AIR V Low profile roof air



Windows, Forward, Diamond Seaglaze, 2-D5 fixed, 1-(center)“Safari” Top hinge 



opening



Windows, side, 2 each side, sliding, Diamond Seaglaze 106S


Windows, rear, 2, Diamond Seaglaze D5 fixed


Entry door, heavy duty aluminum, Diamond Seaglaze, with drop-slide window and




stainless Trio-Ving deadbolt lockset



Windshield wipers, Imtra, Roca, self parking with AFI stainless pantograph arms



Screens on all opening windows and portlites


Companion seats, 2-Bentleys Rivermaster, portside forward with folding armrests



Convertible dinette portside aft with drawers under



Headliner, soft touch with acoustic foam insulation and 4 cabin lights, (red/white)


Lighting; Galley, Remote control, dimmable LED in headliner



Heavy duty rubber flooring



Window covers



Teak trim 
NOTE;


All interior framing for all cabinetry and components are constructed of aluminum,


welded in place to the hull structure for maximum strength and durability.
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Flying Bridge

Cabin roof reinforcement


1/8” 5052 treadplate roof


Tall fold down arch with Radar, GPS, VHF antenna, spotlight and satellite dome 
mounts


Flying bridge hand rails and ladder


2-Bentleys Guide helmseats with fixed arms


Wind deflector for comfortable cruising


Console with hydraulic steering, Volvo EVC controls, EVC tachometers with


engine and fuel data EVC drive trim and trim tab control


Huge storage area under console with 2 Bomar hatch access

Sunbrella covers for seats and instrument console


Tie downs for dinghy
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Electronics

Main helm;



Radar/ chartplotter


Furuno 1834C-NT 36 mile (4kw) 











with radar/chartplotter overlay



Auxiliary display



Furuno GP 1720C-NT



Sounder 





Furuno BBFF3 (3000 watt)



Transducer 




Furuno 2000W,CA 50/200ID R199 (In Hull)



Transducer matching box

Furuno MB 1000



Heading Sensor



Furuno PG500



Network Hub



VHF






ICOM M-604



VHF antenna




Shakespeare 5225 Galaxy



Compass





KVH Azimuth 1000 electronic



Stereo






Alpine


Speakers





PolyPlanar MA905 (4) recessed in headliner

Aft station



Auxiliary display 



Furuno GP 1720C-NT on RAM swivel mount



VHF






ICOM HM 162 Command Mic

Flybridge





Auxiliary display



Furuno GP 1720C-NT



VHF






ICOM HM 162 Command Mic



Compass





Ritchie SS 2000 magnetic



Satellite TV 




KVH TV1
